**HEARING AID ON A MOULD**

**A BASIC GUIDE**

**Elbow .** This connects the aid to the tube. There are various different sizes depending on the aid.



 

**Various types of hearing aid are provided on a mould but these all have an elbow to connect the tube of a mould to the aid.**

 

Moulds should be washed in warm soapy water at least once a week, then dried out by shaking water out and leaving on a dry surface, before being connected back to the aid. They should not be placed on a radiator etc.

**Tube.** There are different thicknesses and materials a tube can be made from.

**MOULD.** There are different types and materials of mould.



The tube and elbow push together to connect them.

This will become difficult to attach/ disconnect as the tube gets old so it MUST be replaced at least every 6months



